***Teraterm serial logs***

Or new connection we need to set the

1)serial option.

2)port COM4 USB serial port

Later in options we need to set baud rate

Setup – serial port – speed (115200)

Later we need to reboot the device.

We will get the serial logs from board level.