Step 1: put the device in fastboot mode

Step 2: Run .bat file to erase partitions

Step 3: flash images using QFIL

Step 4: put the device in fastboot mode

erase userdata , enterprise , factory

step 5: reboot and again fastboot

fastboot flash persist persist.img

fastboot flash enterprise enterprise.img

fastboot flash factory factory.img

step 6: reboot the device.

To flash NON-HLOS\_WLAN.bin

Command:

fastboot flash modem\_a NON-HLOS\_WLAN.bin